#MicroXplorer Configuration settings - do not modify
ADC1.AWD1HighThreshold=1828
ADC1.AWD1ITMode=ENABLE
ADC1.AWD1LowThreshold=1721
ADC1.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_TEMPSENSOR
ADC1.Channel-1\#ChannelRegularConversion=ADC_CHANNEL_VREFINT
ADC1.Channel-2\#ChannelRegularConversion=ADC_CHANNEL_3
ADC1.Channel-3\#ChannelRegularConversion=ADC_CHANNEL_4
ADC1.Channel-4\#ChannelRegularConversion=ADC_CHANNEL_5
ADC1.Channel-5\#ChannelRegularConversion=ADC_CHANNEL_6
ADC1.Channel-6\#ChannelRegularConversion=ADC_CHANNEL_7
ADC1.ContinuousConvMode=ENABLE
ADC1.EnableAnalogWatchDog=true
ADC1.ExternalTrigConv=ADC_SOFTWARE_START
ADC1.IPParameters=Rank-0\#ChannelRegularConversion,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,NbrOfConversionFlag,ContinuousConvMode,Rank-1\#ChannelRegularConversion,Channel-1\#ChannelRegularConversion,SamplingTime-1\#ChannelRegularConversion,Rank-2\#ChannelRegularConversion,Channel-2\#ChannelRegularConversion,SamplingTime-2\#ChannelRegularConversion,Rank-3\#ChannelRegularConversion,Channel-3\#ChannelRegularConversion,SamplingTime-3\#ChannelRegularConversion,NbrOfConversion,Rank-4\#ChannelRegularConversion,Channel-4\#ChannelRegularConversion,SamplingTime-4\#ChannelRegularConversion,Rank-5\#ChannelRegularConversion,Channel-5\#ChannelRegularConversion,SamplingTime-5\#ChannelRegularConversion,ExternalTrigConv,master,EnableAnalogWatchDog,Rank-6\#ChannelRegularConversion,Channel-6\#ChannelRegularConversion,SamplingTime-6\#ChannelRegularConversion,WatchdogMode,AWD1ITMode,WatchdogChannel,AWD1HighThreshold,AWD1LowThreshold
ADC1.NbrOfConversion=7
ADC1.NbrOfConversionFlag=1
ADC1.Rank-0\#ChannelRegularConversion=1
ADC1.Rank-1\#ChannelRegularConversion=2
ADC1.Rank-2\#ChannelRegularConversion=3
ADC1.Rank-3\#ChannelRegularConversion=4
ADC1.Rank-4\#ChannelRegularConversion=5
ADC1.Rank-5\#ChannelRegularConversion=6
ADC1.Rank-6\#ChannelRegularConversion=7
ADC1.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_239CYCLES_5
ADC1.SamplingTime-1\#ChannelRegularConversion=ADC_SAMPLETIME_239CYCLES_5
ADC1.SamplingTime-2\#ChannelRegularConversion=ADC_SAMPLETIME_239CYCLES_5
ADC1.SamplingTime-3\#ChannelRegularConversion=ADC_SAMPLETIME_239CYCLES_5
ADC1.SamplingTime-4\#ChannelRegularConversion=ADC_SAMPLETIME_239CYCLES_5
ADC1.SamplingTime-5\#ChannelRegularConversion=ADC_SAMPLETIME_239CYCLES_5
ADC1.SamplingTime-6\#ChannelRegularConversion=ADC_SAMPLETIME_239CYCLES_5
ADC1.WatchdogChannel=ADC_CHANNEL_TEMPSENSOR
ADC1.WatchdogMode=ADC_ANALOGWATCHDOG_SINGLE_REG
ADC1.master=1
ARM.CMSIS.5.6.0.CMSISJjDSP=Library
ARM.CMSIS.5.6.0.CMSISJjNNOoLib=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjCANJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjEthernetJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjEthernetOoMACJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjEthernetOoPHYJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjFlashJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjI2CJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjMCIJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjNANDJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjSAIJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjSPIJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjUSARTJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjUSBOoDeviceJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjUSBOoDevice_Checked=false
ARM.CMSIS.5.6.0.CMSISOoDriverJjUSBOoHostJjCustom=true
ARM.CMSIS.5.6.0.CMSISOoDriverJjWiFiJjCustom=true
ARM.CMSIS.5.6.0.DeviceJjIRQOoControllerJjGIC=true
ARM.CMSIS.5.6.0.DeviceJjOSOoTickJjPrivateOoTimer=true
ARM.CMSIS.5.6.0.DeviceJjStartup=COoStartup
ARM.CMSIS.5.6.0.IPParameters=CMSISJjNNOoLib,DeviceJjIRQOoControllerJjGIC,DeviceJjOSOoTickJjPrivateOoTimer,CMSISOoDriverJjUSARTJjCustom,CMSISOoDriverJjSPIJjCustom,CMSISOoDriverJjSAIJjCustom,CMSISOoDriverJjI2CJjCustom,CMSISOoDriverJjCANJjCustom,CMSISOoDriverJjFlashJjCustom,CMSISOoDriverJjMCIJjCustom,CMSISOoDriverJjNANDJjCustom,CMSISOoDriverJjEthernetJjCustom,CMSISOoDriverJjEthernetOoMACJjCustom,CMSISOoDriverJjEthernetOoPHYJjCustom,CMSISOoDriverJjUSBOoDeviceJjCustom,CMSISOoDriverJjUSBOoHostJjCustom,CMSISOoDriverJjWiFiJjCustom,CMSISJjDSP,DeviceJjStartup
ARM.CMSIS.5.6.0_SwParameter=CMSISOoDriverJjUSARTJjCustom\:true;DeviceJjOSOoTickJjPrivateOoTimer\:true;CMSISOoDriverJjUSBOoDeviceJjCustom\:true;CMSISOoDriverJjCANJjCustom\:true;CMSISOoDriverJjFlashJjCustom\:true;CMSISOoDriverJjNANDJjCustom\:true;CMSISOoDriverJjEthernetJjCustom\:true;CMSISOoDriverJjEthernetOoMACJjCustom\:true;CMSISOoDriverJjUSBOoHostJjCustom\:true;CMSISOoDriverJjSAIJjCustom\:true;CMSISOoDriverJjWiFiJjCustom\:true;CMSISJjDSP\:Library;CMSISOoDriverJjSPIJjCustom\:true;CMSISOoDriverJjMCIJjCustom\:true;CMSISOoDriverJjEthernetOoPHYJjCustom\:true;DeviceJjIRQOoControllerJjGIC\:true;CMSISJjNNOoLib\:true;DeviceJjStartup\:COoStartup;CMSISOoDriverJjI2CJjCustom\:true;
Dma.ADC1.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC1.0.Instance=DMA1_Channel1
Dma.ADC1.0.MemDataAlignment=DMA_MDATAALIGN_WORD
Dma.ADC1.0.MemInc=DMA_MINC_ENABLE
Dma.ADC1.0.Mode=DMA_CIRCULAR
Dma.ADC1.0.PeriphDataAlignment=DMA_PDATAALIGN_WORD
Dma.ADC1.0.PeriphInc=DMA_PINC_DISABLE
Dma.ADC1.0.Priority=DMA_PRIORITY_LOW
Dma.ADC1.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority
Dma.Request0=ADC1
Dma.RequestsNb=1
FREERTOS.FootprintOK=true
FREERTOS.HEAP_NUMBER=4
FREERTOS.INCLUDE_pcTaskGetTaskName=1
FREERTOS.INCLUDE_vTaskCleanUpResources=1
FREERTOS.INCLUDE_xEventGroupSetBitFromISR=1
FREERTOS.INCLUDE_xSemaphoreGetMutexHolder=1
FREERTOS.INCLUDE_xTaskAbortDelay=1
FREERTOS.INCLUDE_xTaskGetCurrentTaskHandle=1
FREERTOS.INCLUDE_xTaskGetHandle=1
FREERTOS.IPParameters=Tasks01,configMAX_TASK_NAME_LEN,configUSE_TICKLESS_IDLE,INCLUDE_xTaskGetCurrentTaskHandle,INCLUDE_xTaskGetHandle,configUSE_APPLICATION_TASK_TAG,FootprintOK,configUSE_IDLE_HOOK,configUSE_TICK_HOOK,configUSE_MALLOC_FAILED_HOOK,configGENERATE_RUN_TIME_STATS,configUSE_STATS_FORMATTING_FUNCTIONS,configUSE_TRACE_FACILITY,HEAP_NUMBER,configTOTAL_HEAP_SIZE,configCHECK_FOR_STACK_OVERFLOW,configUSE_TASK_NOTIFICATIONS,INCLUDE_xTaskAbortDelay,INCLUDE_xEventGroupSetBitFromISR,INCLUDE_xSemaphoreGetMutexHolder,INCLUDE_pcTaskGetTaskName,INCLUDE_vTaskCleanUpResources
FREERTOS.Tasks01=defaultTask,24,128,StartDefaultTask,Default,NULL,Dynamic,NULL,NULL;LedBlinkTask,8,128,StartLedBlinkTask,Default,NULL,Dynamic,NULL,NULL;CoulombRead,8,128,StartCoulombRead,Default,NULL,Dynamic,NULL,NULL;PowerMonitTask,8,128,StartPowerMonitTask,Default,NULL,Dynamic,NULL,NULL;EventDetect,8,128,StartEventDetect,Default,NULL,Dynamic,NULL,NULL
FREERTOS.configCHECK_FOR_STACK_OVERFLOW=1
FREERTOS.configGENERATE_RUN_TIME_STATS=1
FREERTOS.configMAX_TASK_NAME_LEN=32
FREERTOS.configTOTAL_HEAP_SIZE=8192
FREERTOS.configUSE_APPLICATION_TASK_TAG=0
FREERTOS.configUSE_IDLE_HOOK=1
FREERTOS.configUSE_MALLOC_FAILED_HOOK=0
FREERTOS.configUSE_STATS_FORMATTING_FUNCTIONS=0
FREERTOS.configUSE_TASK_NOTIFICATIONS=1
FREERTOS.configUSE_TICKLESS_IDLE=1
FREERTOS.configUSE_TICK_HOOK=1
FREERTOS.configUSE_TRACE_FACILITY=0
File.Version=6
GPIO.groupedBy=Group By Peripherals
IWDG.IPParameters=Prescaler,Reload
IWDG.Prescaler=IWDG_PRESCALER_16
IWDG.Reload=0xfff
KeepUserPlacement=false
Mcu.Family=STM32F1
Mcu.IP0=ADC1
Mcu.IP1=DMA
Mcu.IP10=USART1
Mcu.IP11=USB_DEVICE
Mcu.IP12=USB_OTG_FS
Mcu.IP2=FREERTOS
Mcu.IP3=I2C1
Mcu.IP4=IWDG
Mcu.IP5=NVIC
Mcu.IP6=RCC
Mcu.IP7=RTC
Mcu.IP8=SYS
Mcu.IP9=UART4
Mcu.IPNb=13
Mcu.Name=STM32F107V(B-C)Tx
Mcu.Package=LQFP100
Mcu.Pin0=PE2
Mcu.Pin1=PE3
Mcu.Pin10=PC3
Mcu.Pin11=PA0-WKUP
Mcu.Pin12=PA3
Mcu.Pin13=PA4
Mcu.Pin14=PA5
Mcu.Pin15=PA6
Mcu.Pin16=PA7
Mcu.Pin17=PC4
Mcu.Pin18=PC5
Mcu.Pin19=PE8
Mcu.Pin2=PE4
Mcu.Pin20=PE9
Mcu.Pin21=PE10
Mcu.Pin22=PE11
Mcu.Pin23=PE12
Mcu.Pin24=PE13
Mcu.Pin25=PB10
Mcu.Pin26=PB11
Mcu.Pin27=PB12
Mcu.Pin28=PB13
Mcu.Pin29=PB14
Mcu.Pin3=PE5
Mcu.Pin30=PB15
Mcu.Pin31=PD8
Mcu.Pin32=PD9
Mcu.Pin33=PD10
Mcu.Pin34=PD11
Mcu.Pin35=PD12
Mcu.Pin36=PD13
Mcu.Pin37=PD14
Mcu.Pin38=PD15
Mcu.Pin39=PC6
Mcu.Pin4=PE6
Mcu.Pin40=PC7
Mcu.Pin41=PC8
Mcu.Pin42=PA8
Mcu.Pin43=PA9
Mcu.Pin44=PA10
Mcu.Pin45=PA11
Mcu.Pin46=PA12
Mcu.Pin47=PA13
Mcu.Pin48=PA14
Mcu.Pin49=PC10
Mcu.Pin5=OSC_IN
Mcu.Pin50=PC11
Mcu.Pin51=PC12
Mcu.Pin52=PD0
Mcu.Pin53=PD1
Mcu.Pin54=PD2
Mcu.Pin55=PD3
Mcu.Pin56=PD4
Mcu.Pin57=PD5
Mcu.Pin58=PD6
Mcu.Pin59=PD7
Mcu.Pin6=OSC_OUT
Mcu.Pin60=PB3
Mcu.Pin61=PB4
Mcu.Pin62=PB5
Mcu.Pin63=PB8
Mcu.Pin64=PB9
Mcu.Pin65=VP_ADC1_TempSens_Input
Mcu.Pin66=VP_ADC1_Vref_Input
Mcu.Pin67=VP_FREERTOS_VS_CMSIS_V2
Mcu.Pin68=VP_IWDG_VS_IWDG
Mcu.Pin69=VP_RTC_VS_RTC_Activate
Mcu.Pin7=PC0
Mcu.Pin70=VP_SYS_VS_tim1
Mcu.Pin71=VP_USB_DEVICE_VS_USB_DEVICE_CDC_FS
Mcu.Pin8=PC1
Mcu.Pin9=PC2
Mcu.PinsNb=72
Mcu.ThirdParty0=ARM.CMSIS.5.6.0
Mcu.ThirdPartyNb=1
Mcu.UserConstants=
Mcu.UserName=STM32F107VCTx
MxCube.Version=6.1.0
MxDb.Version=DB.6.0.10
NVIC.ADC1_2_IRQn=true\:5\:0\:false\:true\:true\:8\:true\:true\:true
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.DMA1_Channel1_IRQn=true\:5\:0\:false\:true\:true\:9\:true\:false\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:true\:false\:true\:false\:false\:false
NVIC.EXTI0_IRQn=true\:5\:0\:false\:true\:true\:11\:true\:true\:true
NVIC.EXTI3_IRQn=true\:5\:0\:false\:true\:true\:12\:true\:true\:true
NVIC.EXTI4_IRQn=true\:5\:0\:false\:true\:true\:16\:true\:true\:true
NVIC.EXTI9_5_IRQn=true\:5\:0\:true\:true\:true\:13\:true\:true\:true
NVIC.FLASH_IRQn=true\:5\:0\:false\:true\:true\:2\:true\:true\:true
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.I2C1_ER_IRQn=true\:5\:0\:true\:true\:true\:7\:false\:true\:true
NVIC.I2C1_EV_IRQn=true\:5\:0\:false\:true\:true\:6\:true\:true\:true
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.OTG_FS_IRQn=true\:5\:0\:false\:true\:true\:4\:true\:false\:true
NVIC.PVD_IRQn=true\:5\:0\:true\:true\:true\:1\:false\:true\:true
NVIC.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.RCC_IRQn=true\:5\:0\:false\:true\:true\:3\:true\:true\:false
NVIC.RTC_Alarm_IRQn=true\:5\:0\:false\:true\:true\:14\:true\:true\:true
NVIC.RTC_IRQn=true\:5\:0\:false\:true\:true\:15\:true\:true\:true
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false\:false
NVIC.SavedPendsvIrqHandlerGenerated=true
NVIC.SavedSvcallIrqHandlerGenerated=true
NVIC.SavedSystickIrqHandlerGenerated=true
NVIC.SysTick_IRQn=true\:15\:0\:false\:false\:false\:true\:false\:true
NVIC.TIM1_UP_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:true
NVIC.TimeBase=TIM1_UP_IRQn
NVIC.TimeBaseIP=TIM1
NVIC.UART4_IRQn=true\:5\:0\:false\:true\:true\:5\:true\:true\:true
NVIC.USART1_IRQn=true\:5\:0\:false\:true\:true\:10\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
OSC_IN.Mode=HSE-External-Oscillator
OSC_IN.Signal=RCC_OSC_IN
OSC_OUT.Mode=HSE-External-Oscillator
OSC_OUT.Signal=RCC_OSC_OUT
PA0-WKUP.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultEXTI
PA0-WKUP.GPIO_Label=SYS_POWER_BTN
PA0-WKUP.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_RISING_FALLING
PA0-WKUP.GPIO_PuPd=GPIO_PULLDOWN
PA0-WKUP.Locked=true
PA0-WKUP.Signal=GPXTI0
PA10.Locked=true
PA10.Mode=Asynchronous
PA10.Signal=USART1_RX
PA11.GPIOParameters=GPIO_Label
PA11.GPIO_Label=USB2_FS_DM
PA11.Locked=true
PA11.Mode=Device_Only
PA11.Signal=USB_OTG_FS_DM
PA12.GPIOParameters=GPIO_Label
PA12.GPIO_Label=USB2_FS_DP
PA12.Locked=true
PA12.Mode=Device_Only
PA12.Signal=USB_OTG_FS_DP
PA13.GPIOParameters=GPIO_Label
PA13.GPIO_Label=SYS_SWDIO
PA13.Locked=true
PA13.Mode=Trace_Asynchronous_SW
PA13.Signal=SYS_JTMS-SWDIO
PA14.GPIOParameters=GPIO_Label
PA14.GPIO_Label=SYS_SWCLK
PA14.Locked=true
PA14.Mode=Trace_Asynchronous_SW
PA14.Signal=SYS_JTCK-SWCLK
PA3.GPIOParameters=GPIO_Label
PA3.GPIO_Label=MON_24V0_DIV16
PA3.Locked=true
PA3.Signal=ADCx_IN3
PA4.GPIOParameters=GPIO_Label
PA4.GPIO_Label=MON_5V0_DIV8
PA4.Locked=true
PA4.Signal=ADCx_IN4
PA5.GPIOParameters=GPIO_Label
PA5.GPIO_Label=MON_12V0_DIV8
PA5.Locked=true
PA5.Signal=ADCx_IN5
PA6.GPIOParameters=GPIO_Label
PA6.GPIO_Label=MON_BKP_BAT_DIV8
PA6.Locked=true
PA6.Signal=ADCx_IN6
PA7.GPIOParameters=GPIO_Label
PA7.GPIO_Label=MON_MAIN_PWR_DIV16
PA7.Locked=true
PA7.Signal=ADCx_IN7
PA8.GPIOParameters=PinState,GPIO_Label,GPIO_ModeDefaultOutputPP
PA8.GPIO_Label=USB2_FS_ENUM_CTL
PA8.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_PP
PA8.Locked=true
PA8.PinState=GPIO_PIN_RESET
PA8.Signal=GPIO_Output
PA9.Locked=true
PA9.Mode=Asynchronous
PA9.Signal=USART1_TX
PB10.GPIOParameters=GPIO_Label
PB10.GPIO_Label=IIC2_SCL
PB10.Locked=true
PB10.Signal=GPIO_Output
PB11.GPIOParameters=GPIO_Label
PB11.GPIO_Label=IIC2_SDA
PB11.Locked=true
PB11.Signal=GPIO_Output
PB12.GPIOParameters=GPIO_Label
PB12.GPIO_Label=USB2_VBUS_CTL_1
PB12.Locked=true
PB12.Signal=GPIO_Output
PB13.GPIOParameters=GPIO_Label
PB13.GPIO_Label=USB2_VBUS_CTL_2
PB13.Locked=true
PB13.Signal=GPIO_Output
PB14.GPIOParameters=GPIO_Label
PB14.GPIO_Label=USB2_VBUS_CTL_3
PB14.Locked=true
PB14.Signal=GPIO_Output
PB15.GPIOParameters=GPIO_Label
PB15.GPIO_Label=USB2_VBUS_CTL_4
PB15.Locked=true
PB15.Signal=GPIO_Output
PB3.GPIOParameters=GPIO_Label
PB3.GPIO_Label=SYS_SWO
PB3.Mode=Trace_Asynchronous_SW
PB3.Signal=SYS_TRACESWO
PB4.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultEXTI
PB4.GPIO_Label=SOM_MOD_SLEEP
PB4.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_RISING_FALLING
PB4.GPIO_PuPd=GPIO_PULLUP
PB4.Locked=true
PB4.Signal=GPXTI4
PB5.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultOutputPP
PB5.GPIO_Label=SOM_SYS_RESET
PB5.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PB5.GPIO_PuPd=GPIO_PULLUP
PB5.Locked=true
PB5.Signal=GPIO_Output
PB8.GPIOParameters=GPIO_Label
PB8.GPIO_Label=IIC1_SCL
PB8.Locked=true
PB8.Mode=I2C
PB8.Signal=I2C1_SCL
PB9.GPIOParameters=GPIO_Label
PB9.GPIO_Label=IIC1_SDA
PB9.Locked=true
PB9.Mode=I2C
PB9.Signal=I2C1_SDA
PC0.GPIOParameters=PinState,GPIO_Label
PC0.GPIO_Label=PMB_CHRG_SHDN
PC0.Locked=true
PC0.PinState=GPIO_PIN_SET
PC0.Signal=GPIO_Output
PC1.GPIOParameters=GPIO_Label
PC1.GPIO_Label=PMB_TEMP_SEN_EN
PC1.Locked=true
PC1.Signal=GPIO_Output
PC10.Locked=true
PC10.Mode=Asynchronous
PC10.Signal=UART4_TX
PC11.Locked=true
PC11.Mode=Asynchronous
PC11.Signal=UART4_RX
PC12.GPIOParameters=GPIO_Label
PC12.GPIO_Label=SOC_U2_HUB_PWR_CTL
PC12.Locked=true
PC12.Signal=GPIO_Output
PC2.GPIOParameters=GPIO_Label
PC2.GPIO_Label=PMB_TEMP_SEN_ALT
PC2.Locked=true
PC2.Signal=GPIO_Input
PC3.GPIOParameters=GPIO_Label
PC3.GPIO_Label=PMB_CLOULOMB_ALCC
PC3.Locked=true
PC3.Signal=GPIO_Input
PC4.GPIOParameters=GPIO_Label
PC4.GPIO_Label=SYS_RUN_LED_CTL
PC4.Locked=true
PC4.Signal=GPIO_Output
PC5.GPIOParameters=PinState,GPIO_Label
PC5.GPIO_Label=SYS_BUZZ_CTL
PC5.Locked=true
PC5.PinState=GPIO_PIN_SET
PC5.Signal=GPIO_Output
PC6.GPIOParameters=GPIO_Label
PC6.GPIO_Label=SOC_U3_HOST_PWR_STA
PC6.Locked=true
PC6.Signal=GPXTI6
PC7.GPIOParameters=GPIO_Label
PC7.GPIO_Label=SOC_U3_HUB_PWR_STA
PC7.Locked=true
PC7.Signal=GPXTI7
PC8.GPIOParameters=GPIO_Label
PC8.GPIO_Label=SOC_U2_HUB_PWR_STA
PC8.Locked=true
PC8.Signal=GPXTI8
PCC.Checker=false
PCC.Line=STM32F105/107
PCC.MCU=STM32F107V(B-C)Tx
PCC.PartNumber=STM32F107VCTx
PCC.Seq0=2
PCC.Seq0.Step0.Average_Current=14.8 mA
PCC.Seq0.Step0.CPU_Frequency=36 MHz
PCC.Seq0.Step0.Category=In DS Table
PCC.Seq0.Step0.DMIPS=45.0
PCC.Seq0.Step0.Duration=0.1 ms
PCC.Seq0.Step0.Frequency=8 MHz
PCC.Seq0.Step0.Memory=FLASH
PCC.Seq0.Step0.Mode=RUN
PCC.Seq0.Step0.Oscillator=HSI PLL
PCC.Seq0.Step0.Peripherals=
PCC.Seq0.Step0.TaMax=102.75
PCC.Seq0.Step0.User's_Consumption=0 mA
PCC.Seq0.Step0.Vcore=No Scale
PCC.Seq0.Step0.Vdd=3.3
PCC.Seq0.Step0.Voltage_Source=Battery
PCC.Seq0.Step1.Average_Current=26 \u00B5A
PCC.Seq0.Step1.CPU_Frequency=0 Hz
PCC.Seq0.Step1.Category=In DS Table
PCC.Seq0.Step1.DMIPS=0.0
PCC.Seq0.Step1.Duration=0.9 ms
PCC.Seq0.Step1.Frequency=0 Hz
PCC.Seq0.Step1.Memory=n/a
PCC.Seq0.Step1.Mode=STOP
PCC.Seq0.Step1.Oscillator=Regulator_LP
PCC.Seq0.Step1.Peripherals=
PCC.Seq0.Step1.TaMax=105
PCC.Seq0.Step1.User's_Consumption=0 mA
PCC.Seq0.Step1.Vcore=No Scale
PCC.Seq0.Step1.Vdd=3.3
PCC.Seq0.Step1.Voltage_Source=Battery
PCC.Series=STM32F1
PCC.Temperature=25
PCC.Vdd=3.3
PD0.GPIOParameters=GPIO_Label
PD0.GPIO_Label=SOC_U3_HUB_PWR_CTL
PD0.Locked=true
PD0.Signal=GPIO_Output
PD1.GPIOParameters=GPIO_Label
PD1.GPIO_Label=SOC_U3_HOST_PWR_CTL
PD1.Locked=true
PD1.Signal=GPIO_Output
PD10.GPIOParameters=GPIO_Label
PD10.GPIO_Label=USB3_VBUS_CTL_5
PD10.Locked=true
PD10.Signal=GPIO_Output
PD11.GPIOParameters=GPIO_Label
PD11.GPIO_Label=USB3_VBUS_CTL_6
PD11.Locked=true
PD11.Signal=GPIO_Output
PD12.GPIOParameters=GPIO_Label
PD12.GPIO_Label=USB3_VBUS_CTL_1
PD12.Locked=true
PD12.Signal=GPIO_Output
PD13.GPIOParameters=GPIO_Label
PD13.GPIO_Label=USB3_VBUS_CTL_2
PD13.Locked=true
PD13.Signal=GPIO_Output
PD14.GPIOParameters=GPIO_Label
PD14.GPIO_Label=USB3_VBUS_CTL_3
PD14.Locked=true
PD14.Signal=GPIO_Output
PD15.GPIOParameters=GPIO_Label
PD15.GPIO_Label=USB3_VBUS_CTL_4
PD15.Locked=true
PD15.Signal=GPIO_Output
PD2.GPIOParameters=GPIO_Label
PD2.GPIO_Label=SOC_U3_GEC_PWR_CTL
PD2.Locked=true
PD2.Signal=GPIO_Output
PD3.GPIOParameters=GPIO_Label
PD3.GPIO_Label=SOC_GE_SW_PWR_CTL
PD3.Locked=true
PD3.Signal=GPIO_Output
PD4.GPIOParameters=GPIO_Label
PD4.GPIO_Label=SOM_POWER_EN
PD4.Locked=true
PD4.Signal=GPIO_Output
PD5.GPIOParameters=GPIO_Label,GPIO_ModeDefaultEXTI
PD5.GPIO_Label=SOM_SHUTDOWN_REQ
PD5.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_RISING_FALLING
PD5.Locked=true
PD5.Signal=GPXTI5
PD6.GPIOParameters=PinState,GPIO_Label
PD6.GPIO_Label=SOM_SLEEP_WAKE
PD6.Locked=true
PD6.PinState=GPIO_PIN_SET
PD6.Signal=GPIO_Output
PD7.GPIOParameters=PinState,GPIO_Label
PD7.GPIO_Label=SOM_FORCE_RECOVERY
PD7.Locked=true
PD7.PinState=GPIO_PIN_SET
PD7.Signal=GPIO_Output
PD8.GPIOParameters=GPIO_Label
PD8.GPIO_Label=USB2_VBUS_CTL_5
PD8.Locked=true
PD8.Signal=GPIO_Output
PD9.GPIOParameters=GPIO_Label
PD9.GPIO_Label=USB2_VBUS_CTL_6
PD9.Locked=true
PD9.Signal=GPIO_Output
PE10.GPIOParameters=GPIO_Label
PE10.GPIO_Label=SYS_FAN_CTL_2
PE10.Locked=true
PE10.Signal=GPIO_Output
PE11.GPIOParameters=GPIO_Label
PE11.GPIO_Label=SYS_FAN_SNS_2
PE11.Locked=true
PE11.Signal=GPIO_Input
PE12.GPIOParameters=GPIO_Label
PE12.GPIO_Label=SYS_FAN_CTL_3
PE12.Locked=true
PE12.Signal=GPIO_Output
PE13.GPIOParameters=GPIO_Label
PE13.GPIO_Label=SYS_FAN_SNS_3
PE13.Locked=true
PE13.Signal=GPIO_Input
PE2.GPIOParameters=PinState,GPIO_Label
PE2.GPIO_Label=SYS_POWER_LED_CTL
PE2.Locked=true
PE2.PinState=GPIO_PIN_SET
PE2.Signal=GPIO_Output
PE3.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultEXTI
PE3.GPIO_Label=SYS_CUSTOM_BTN
PE3.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_RISING_FALLING
PE3.GPIO_PuPd=GPIO_PULLUP
PE3.Locked=true
PE3.Signal=GPXTI3
PE4.GPIOParameters=GPIO_Label
PE4.GPIO_Label=PMB_PS_ON
PE4.Locked=true
PE4.Signal=GPIO_Output
PE5.GPIOParameters=GPIO_PuPd,GPIO_Label
PE5.GPIO_Label=PMB_CHRG_STAT2
PE5.GPIO_PuPd=GPIO_PULLUP
PE5.Locked=true
PE5.Signal=GPIO_Input
PE6.GPIOParameters=GPIO_PuPd,GPIO_Label
PE6.GPIO_Label=PMB_CHRG_STAT1
PE6.GPIO_PuPd=GPIO_PULLUP
PE6.Locked=true
PE6.Signal=GPIO_Input
PE8.GPIOParameters=GPIO_Label
PE8.GPIO_Label=SYS_FAN_CTL_1
PE8.Locked=true
PE8.Signal=GPIO_Output
PE9.GPIOParameters=GPIO_Label
PE9.GPIO_Label=SYS_FAN_SNS_1
PE9.Locked=true
PE9.Signal=GPIO_Input
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=true
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32F107VCTx
ProjectManager.FirmwarePackage=STM32Cube FW_F1 V1.8.3
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x400
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=NaviKit_stm32.ioc
ProjectManager.ProjectName=NaviKit_stm32
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x800
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-HAL-true,2-MX_DMA_Init-DMA-false-HAL-true,3-SystemClock_Config-RCC-false-HAL-true,4-MX_USB_DEVICE_Init-USB_DEVICE-false-HAL-false,5-MX_I2C1_Init-I2C1-false-HAL-true,6-MX_IWDG_Init-IWDG-false-HAL-true,7-MX_UART4_Init-UART4-false-HAL-true,8-MX_ADC1_Init-ADC1-false-HAL-true,9-MX_USART1_UART_Init-USART1-false-HAL-true,10-MX_RTC_Init-RTC-false-HAL-true
RCC.ADCFreqValue=140625
RCC.ADCPresc=RCC_ADCPCLK2_DIV8
RCC.AHBCLKDivider=RCC_SYSCLK_DIV4
RCC.AHBFreq_Value=18000000
RCC.APB1CLKDivider=RCC_HCLK_DIV16
RCC.APB1Freq_Value=1125000
RCC.APB1TimFreq_Value=2250000
RCC.APB2CLKDivider=RCC_HCLK_DIV16
RCC.APB2Freq_Value=1125000
RCC.APB2TimFreq_Value=2250000
RCC.FCLKCortexFreq_Value=18000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=18000000
RCC.HSE_VALUE=12000000
RCC.I2S2Freq_Value=72000000
RCC.I2S3Freq_Value=72000000
RCC.IPParameters=ADCFreqValue,ADCPresc,AHBCLKDivider,AHBFreq_Value,APB1CLKDivider,APB1Freq_Value,APB1TimFreq_Value,APB2CLKDivider,APB2Freq_Value,APB2TimFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,I2S2Freq_Value,I2S3Freq_Value,MCOFreq_Value,PLL2CLKoutputFreqValue,PLL2VCOoutputFreqValue,PLL3CLKoutputFreqValue,PLL3VCOoutputFreqValue,PLLCLKFreq_Value,PLLMUL,Prediv2,Prediv2FreqValue,SYSCLKFreq_VALUE,SYSCLKSource,TimSysFreq_Value,TimSys_Div,USBFreq_Value,VCOOutput2Freq_Value
RCC.MCOFreq_Value=72000000
RCC.PLL2CLKoutputFreqValue=6000000
RCC.PLL2VCOoutputFreqValue=12000000
RCC.PLL3CLKoutputFreqValue=6000000
RCC.PLL3VCOoutputFreqValue=12000000
RCC.PLLCLKFreq_Value=72000000
RCC.PLLMUL=RCC_PLL_MUL6
RCC.Prediv2=RCC_HSE_PREDIV2_DIV16
RCC.Prediv2FreqValue=750000
RCC.SYSCLKFreq_VALUE=72000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.TimSysFreq_Value=2250000
RCC.TimSys_Div=SYSTICK_CLKSOURCE_HCLK_DIV8
RCC.USBFreq_Value=48000000
RCC.VCOOutput2Freq_Value=12000000
SH.ADCx_IN3.0=ADC1_IN3,IN3
SH.ADCx_IN3.ConfNb=1
SH.ADCx_IN4.0=ADC1_IN4,IN4
SH.ADCx_IN4.ConfNb=1
SH.ADCx_IN5.0=ADC1_IN5,IN5
SH.ADCx_IN5.ConfNb=1
SH.ADCx_IN6.0=ADC1_IN6,IN6
SH.ADCx_IN6.ConfNb=1
SH.ADCx_IN7.0=ADC1_IN7,IN7
SH.ADCx_IN7.ConfNb=1
SH.GPXTI0.0=GPIO_EXTI0
SH.GPXTI0.ConfNb=1
SH.GPXTI3.0=GPIO_EXTI3
SH.GPXTI3.ConfNb=1
SH.GPXTI4.0=GPIO_EXTI4
SH.GPXTI4.ConfNb=1
SH.GPXTI5.0=GPIO_EXTI5
SH.GPXTI5.ConfNb=1
SH.GPXTI6.0=GPIO_EXTI6
SH.GPXTI6.ConfNb=1
SH.GPXTI7.0=GPIO_EXTI7
SH.GPXTI7.ConfNb=1
SH.GPXTI8.0=GPIO_EXTI8
SH.GPXTI8.ConfNb=1
UART4.BaudRate=56000
UART4.IPParameters=VirtualMode,BaudRate
UART4.IPParametersWithoutCheck=BaudRate
UART4.VirtualMode=Asynchronous
USART1.BaudRate=56000
USART1.IPParameters=VirtualMode,WordLength,BaudRate
USART1.VirtualMode=VM_ASYNC
USART1.WordLength=WORDLENGTH_8B
USB_DEVICE.CLASS_NAME_FS=CDC
USB_DEVICE.IPParameters=VirtualMode,VirtualModeFS,CLASS_NAME_FS,USBD_DEBUG_LEVEL
USB_DEVICE.USBD_DEBUG_LEVEL=3
USB_DEVICE.VirtualMode=Cdc
USB_DEVICE.VirtualModeFS=Cdc_FS
USB_OTG_FS.IPParameters=VirtualMode
USB_OTG_FS.VirtualMode=Device_Only
VP_ADC1_TempSens_Input.Mode=IN-TempSens
VP_ADC1_TempSens_Input.Signal=ADC1_TempSens_Input
VP_ADC1_Vref_Input.Mode=IN-Vrefint
VP_ADC1_Vref_Input.Signal=ADC1_Vref_Input
VP_FREERTOS_VS_CMSIS_V2.Mode=CMSIS_V2
VP_FREERTOS_VS_CMSIS_V2.Signal=FREERTOS_VS_CMSIS_V2
VP_IWDG_VS_IWDG.Mode=IWDG_Activate
VP_IWDG_VS_IWDG.Signal=IWDG_VS_IWDG
VP_RTC_VS_RTC_Activate.Mode=RTC_Enabled
VP_RTC_VS_RTC_Activate.Signal=RTC_VS_RTC_Activate
VP_SYS_VS_tim1.Mode=TIM1
VP_SYS_VS_tim1.Signal=SYS_VS_tim1
VP_USB_DEVICE_VS_USB_DEVICE_CDC_FS.Mode=CDC_FS
VP_USB_DEVICE_VS_USB_DEVICE_CDC_FS.Signal=USB_DEVICE_VS_USB_DEVICE_CDC_FS
board=custom
isbadioc=false
